|  |  |
| --- | --- |
| **Hard\_Fault\_Sample** | ok |
| **PowerDown\_Chk** | ok |
| **Semihost** | ok |
| **Template** | ok |

# \SampleCode\Nu-LB-NANO112

|  |  |
| --- | --- |
| COMMON | Not sample code |
| START\_KIT | ok |

# \SampleCode\NUTINY-EVB-NANO112

|  |  |
| --- | --- |
| COMMON | Not sample code |
| LCD\_DEMO | ok |
| PWRDWN\_DEMO | ok |
| PWRDWN\_LCD\_RTC \_DEMO | ok |
| PWRDWN\_RTC\_DEMO | ok |

# \SampleCode\StdDriver

|  |  |
| --- | --- |
| ACMP\_Sigma\_Delta | OK |
| ACMP\_Slope | OK |
| ADC\_Compare | OK |
| ADC\_ContinuousScan | OK |
| ADC\_PDMA | OK |
| ADC\_Single | OK |
| ADC\_SingleCycleScan | OK |
| ADC\_TimerTrigger | OK |
| CRC\_CCITT | OK |
| FMC\_IAP | OK |
| FMC\_RW | OK |
| GPIO\_IOTest | OK |
| GPIO\_PowerDown | OK |
| I2C\_EEPROM | OK |
| I2C\_Loopback | OK |
| I2C\_Wakeup | OK |
| LCD\_Blinking\_Test | ok |
| LCD\_Pixel\_OnOff\_Test | ok |
| LCD\_Print\_Text\_Test | ok |
| PDMA\_Memory | OK |
| PWM\_Capture | OK |
| PWM\_CapturePDMA | OK |
| PWM\_DeadZone | OK |
| RTC\_Alarm\_Test | ok |
| RTC\_Time\_Display | ok |
| SC\_ReadATR | Ok |
| SC\_ReadSimPhoneBook | Ok |
| SCUART\_TxRx | Ok |
| SPI\_FIFO\_Flash | OK |
| SPI\_LoopBack | OK |
| SPI\_TxRxLoopback\_PDMA | OK |
| SYS\_Control | OK |
| SYS\_PLLClockOutput | OK |
| SYS\_TrimIRC | OK |
| Timer\_Delay | Ok |
| Timer\_EventCounter | Ok |
| Timer\_FreeCountingMode | Ok |
| Timer\_InterTimerTriggerMode | Ok |
| Timer\_Periodic | Ok |
| Timer\_ToggleOut | Ok |
| Timer\_TriggerCountingMode | Ok |
| Timer\_Wakeup | ok |
| UART\_AutoBaudRate | ok |
| UART\_FlowCtrl | ok |
| UART\_IrDA | ok |
| UART\_LIN | ok |
| UART\_PDMA | ok |
| UART\_RS485\_Receive | ok |
| UART\_RS485\_Transmit | ok |
| UART\_Rx\_Wakeup | ok |
| UART\_TxRx\_Function | ok |
| WDT\_Polling | Ok |
| WDT\_Wakeup | Ok |
| WWDT\_Reload | Ok |